PC software for DiegoG3 gas controller.
PC software version 3.0.x.x is full compatible with older gas ECU versions - 1.3x, 1.4x and 1.5x

Changes for PC software 3.0.6.1 (full compatibility with gas controller 30H and Adapter OBD 10B):
--------------------------------
+ Improvments in "Start (F5)" window
	* Add selection for COM port  and Connect button.
	* Add information about software, gas controller and Adapter OBD version.
+ Improvements in communication with gas controller (also working with Adapter OBD).
+ Improving Off-line mode.
+ Added HANA gas injector type.

Changes for PC software 3.0.6.0 (full compatibility with gas controller 30H and Adapter OBD 10B):
--------------------------------
+ Update for the Adapter OBD-1.0B
	+ Improved mechanism for reading the error codes
	+ Improved mechanism for establishing communication with the OBD, and cooperation with more than one OBD controller in the car (cars with automatic transmission).
+ Add a "Start (F5)" window  to facilitate the movement of the softare.
+ Simplification of user interface (less tabs).
+ Show all the basic configuration parameters in one tab "Basic", where are old tabs "Engine" and "Instalation".
+ Option 'Correction when injection system is changed (Mazda)' moved to 'Basic' tab.
+ Option 'Microinjection-type engine' moved to 'Basic' tab.
+ Option 'Minimum and maximum gas injection time' moved to 'Basic' tab.
+ Improvement and simplify the Autocalibration procedure (new window initialization).
+ Improvements in communication with gas controller (also working with Adapter OBD).
+ Improving Off-line mode.
+ Adding a search option ports, retrieving the ports automatically when you change the port number (regular driver search on all available ports).
+ Add Bulgarian language.

Changes for PC software 3.0.5.1 (full compatibility with gas controller 30H and Adapter OBD 10A):
--------------------------------
+ Idle points are visible in both simple and advanced view.
+ Buttons "Clear TEMPLATE" and "Load from file..." are invisible for nonsupporting them versions of gas ECU.
+ Added auto-verification on tab Verification (untypical values of parameters are displayed in red)

Changes for PC software 3.0.5.0 (full compatibility with gas controller 30H and Adapter OBD 10A):
--------------------------------
+ Added information about communication ports into the Windows system
+ Added support for Adapters OBD.

Changes for PC software 3.0.4.3 (full compatibility with gas controller 30G):
--------------------------------
+ Translation modification.
+ Added gas injector: Valtek Type34 and changed control algorithms for the gas injectors.

Changes for PC software 3.0.4.2 (full compatibility with gas controller 30G):
--------------------------------
+ Translation modification.
+ Improvement of the firmware update window

Changes for PC software 3.0.4.1 (full compatibility with gas controller 30G):
--------------------------------
+ Translation modification.
+ Corrections configuration moved to new tab Corrections (F11)
+ Option: Return from cut-off on petrol as a new option for automatic return to GAS mode
+ Option: Min and Max gas injection time
+ Improved program scaling for different resolutions
+ Improved calibration process
+ Modification for gas injector list
+ Sound notification if gas system starts on petrol (3x buzzer beep with 10 sec intervals)
+ Inspection management (Sound notification - 10x buzzer beep after switching to gas)
+ Configuration changes registration (date and computer code for each modification)
+ Vacuum and RPM corrections (changes possibility)
+ Additional correction map (RPM/petrol injection time)

Changes for PC software 3.0.3.5 (full compatibility with gas controller 30F):
--------------------------------
+ Modification for gas injector list.

Changes for PC software 3.0.3.4 (full compatibility with gas controller 30F):
--------------------------------
+ Translation modification.

Changes for PC software 3.0.3.3 (full compatibility with gas controller 30F):
--------------------------------
+ Translation modification.
+ Add and remove model points using keyboard.
+ Improved compatibilities with older gas controllers version (1.4x, 1.5x).
+ More precise possibilities of setting the "Earlier valves opening time" parameter to 10 seconds.

Changes for PC software 3.0.3.2 (full compatibility with gas controller 30F):
--------------------------------
+ Added simple and advanced view.
+ Improved Set model function on Map tab.
+ Improved compatibilities with older gas controllers version (1.4x, 1.5x).

Changes for PC software 3.0.3.1 (full compatibility with gas controller 30F):
--------------------------------
+ New function: Enrichment during cut-off about injection _  [ms] if RPM< _.
+ New function: Correction when injection system is changed (Mazda).
+ Added button "Set model" on Map tab (function automatically adjust model regarding to collecting points).
+ Added message that clearing gas map is required when model is writing.
+ New mechanism for injection system detection.
+ Save to file and load from file petrol map template.
+ Moving model points by keyboard is available.
+ Improved Adaptation mechanism.
+ Improved Determining working pressure mechanism.
+ Improved emergency start on gas.
+ Improved fuel overlapping (petro-gas) mechanism (always when system is switching to gas).
+ Improved Gas injectors heating mechanism.
+ Improved nozzles suggestion mechanism.
+ Improved autocalibration mechanism.
+ "RPM sound" active sounds when Tred>40Cdeg. (min temperature for collecting map points).
+ On tab Calibration reducer temperature is displayed on red when Tred<40Cdeg. (min temperature for collecting map points).
+ Notification about possibility of updating the controller (to the most recent firmware).
+ New program manual.

Changes for PC software 3.0.2.5 (full compatibility with gas controller 30E):
--------------------------------
+ Translation modification, 
+ Added “Firmware update” and “Documentation” button on first page of “Configuration wizard”,

Changes for PC software 3.0.2.4 (full compatibility with gas controller 30E):
--------------------------------
+ Solved problem with function "Recalculate model"
+ Improved compatibilities with older gas controllers' versions (1.4x, 1.5x).

Changes for PC software 3.0.2.3 (full compatibility with gas controller 30E):
--------------------------------
+ Added languages: English, Russian, Lithuanian, Czech.
+ Recorder tool improved.
+ Added update file: 30C-20090608.upg.

Changes for PC software 3.0.2.2 (full compatibility with gas controller 30E):
--------------------------------
+ Emergency start on gas improved.
+ Adaptation mode improved.
+ Languages corrections.
+ Improved compatibilities with older gas controllers' versions (1.4x, 1.5x).
+ Added dispay with update file info.
+ Adaptation option moved to tab Calibration(F4)\Modeling\Adaptation.
+ Corrections options (for Tgas and RPM) moved to tab Calibration(F4)\Modeling\Corrections - also for older gas controller versions.

Changes for PC software 3.0.2.1 (full compatibility with gas controller 30D):
--------------------------------
+ !!!New installation package contains software for gas ECU in version 1.3x, 1.4x, 1.5x, 3.0x.!!!

+ Changes in configuration settings detection mechanism.
+ Added pressure configuration for option 'Controll pressure during cut-off.
+ For switching conditions: Switching to PETROL with automatic return to GAS: function 'Tgas<' [Low gas temp.] is changed to 'Tgas< and Load (Petrol)>' [Low gas temp and high Load (Petrol)].
+ Parameters 'Working pressure' and 'Petrol injection time on petrol when idle (no load)' moved from 'Configuration wizard\Installation' to 'Calibration\Modeling'.
+ Improved Autocalibration procedure.
+ Improved Working pressure measuring function.
+ Added gas injectors test.
+ Drawing template line on petrol map after collecting enough petrol points.
+ Added adaptation mechanism for based RPM class.
+ Added model trace.
+ Added possibility of changing correction type for Tgas and RPM.
+ Added firmware update function (menu Device).

Changes for PC software 3.0.1.3 (full compatibility with gas controller 30C):
--------------------------------
+ Displaying of real load percentage depends on the engine injection system type.
+ Windows Vista driver for USB interface added to installation package.
+ New PC software manual.
+ Solved problem with writing default settings for locked device.
+ Changes in displaying of trouble codes.

Changes for PC software 3.0.1.2 (full compatibility with gas controller 30C):
--------------------------------
+ Translation corrections.
+ Added gas injectors: RAIL 2ohms and VALTEK 2ohms.
+ More precise possibilities of setting the "Time for switching a single emulator" parameter: 0; 0,2; 0,4; 0,6; 0,8; 1; 2; 3; 4; 5 (for gasECUs series 1,4 i 1,5 and 30).
+ Vacuum value shown on Calibration pages.

Changes for PC software 3.0.1.1 (full compatibility with gas controller 30C):
-----------------------------------------------
+ New option "RPM wire not connected".
+ Added gas injectors: RAIL IG3 Horizon (E2) i (E3).
+ New option "Gas injectors heating" for low Tred.
+ New option "Fuel overlap (petrol-gas)" with configurable number of cycles and gas injection time.
+ New option Switching to PETROL with automatic return to GAS when Tred to low and high load.
+ New option "Gas pressure control during cut-off".
+ New option "Use model for idle".
+ Function "Set new model" for automatic modelling regarding to idle points..
+ Reset button on Recorder page.
+ Improved Autocalibration procedure.
